The 231221 folder contains an updated collection of PoleNET and associated software for the v3 Agile system. 


---> FOR BEST RESULTS, install the PolenetSuite (or copy all files from its SQ1FW folder to your Polenet SQ1FW folder)


Updated items since previous package 230720:

PoleNET 	      v3.26.52  (Download Host Logs, run Visualiser, Firmware prog speeds, improve Host Monitor)
Agile Base	      v2.75     (Improved resilience and system recovery)
Agile Remote	      v2.75
Agile Remote2x2	      v2.75     (Added ability to operate as a SAF unit)
Agile Logger          v1.28     (Same as v1.27 but comes with Sensor Log Visualiser v1.3.2)
Sensor Log Visualiser v1.3.2    (Show reverse RSSI, Swap between RTUs, larger Chart area, move/zoom individual graphs.)


Items unchanged from previous release package 230720:

Agile Host            v3.29.28  (Improved handling of controllers that use phantom IDs - eg. IrriNet)
Agile DCP             v3.34     (Added support for periodic powered SERIO modbus IOs)
Agile Mux	      v1.09     (Better switching for use as 276 MUX vs 563 Expansion Box, P239 playback)
PoleNET 2 manual      v1.15     (Last updated to show how to map systems with Irrinet controllers)


Other Firmware (included in the Polenet Suite):

Agile Host            v1.98.04  (Playback of inputs greatly improved, bug fixes to log and refresh)
Two-wire Host         v1.58.18  (Handles extreme systems much better, improvements to playback and period calcs)
Two-wire RTU          v1.16
Two-wire RTU          v1.66
Two-wire RTUx8        v3.16     (Updates for revised PCB)


Polenet changes in more detail:

* Added ability to download Logs directly from Host ("System Logs" button)
  - user can choose folder to store logs
    - defaults to new Logs folder inside Polenet folder
    - existing user may prefer to set to folder being used by AgileLogger application (eg. C:\Alog)
  - user can Abort the download before it finishes, without losing the newly downloaded records
  - Polenet reports number of logs currently in Host and how many logs are not yet downloaded in the folder
  - Polenet provides self-adjusting estimate of time remaining to download the fresh log data
  * requires CSVer and logparser in the folder BUT Polenet will auto-install them from SQ1FW folder, if they are there
* Added ability to launch Visualiser (from "System Logs" button, using same Folder)
  * requires Visualiser to be in the folder BUT Polenet will auto-install it from SQ1FW folder, if it is there
* Monitor window obtains base Base TX Power and displays in Network tab
* Monitor window now reports AI Voltages column as actual Voltage (not as an enum)
* Monitor window now reports AI Port_cfg column as "Voltage", "0-5mA", "4-20mA" (not as a complex value)
